# Gravity flow experiment

Last modified by Hannes Bauser on 2022/05/05 19:52
Export
Office Formats
Export as PDF
Other Formats
Export as HTML

Gravity flow experiment, July 2020

Prior to the experiment the NovaLynx tipping buckets were calibrated (see this post).

The experiment was repeated separately for each hillslope, since the storage tanks cannot hold enough water for a 12h rain with the Multi 1 circuit on all 3 hillslopes simultaneously.

For each hillslope a 1h rain event was performed to calibrate the rainfall distribution followed by a 12h rain event on the following day to reach a gravity flow regime down to a depth of 50cm.

Details on the rainfall calibration: rainfall_calibration.xlsx

Schedule:

Date | Task | Comment
--- | --- | ---
| CENTER |
2020-07-06 | Spanned ropes on Center hillslope to mark cup locations for rainfall calibration. | Masts were raised in the morning. Kept raised until after the 12h rain event. Ropes spanned upslope-downslope with pre-labeled marks every 2m from 0-30m.
2020-07-07 | Placed cups on Center hillslope and removed ropes. |
2020-07-08 | Issues with Tipping Bucket counts, switched to cumulative counts to reduce impact. | See also NovaLynx calibration.
2020-07-09 | Rainfall calibration, Multi 1, Center hillslope. Collected and weighed cups after 1h of rain (08:30-09:30). | Details in attached excel file. Air handler off during the rain.
2020-07-10 | 12h rain event (8:30-20:30), Multi 1, Center hillslope. | Air handlers were turned off during rain. Discharge collection for Center -1 (PE102 and NovaLynx) was leaking. Fixed at 19:40. Mast lowered after the rain event.
| EAST |
2020-07-13 | Spanned ropes on East hillslope to mark cup locations for rainfall calibration. | Masts were raised in the morning. Kept raised until after the 12h rain event. Ropes spanned upslope-downslope with pre-labeled marks every 2m from 0-30m.
2020-07-14 | Placed cups on East hillslope and removed ropes. |
2020-07-15 | Rainfall calibration, Multi 1, East hillslope. Collected and weighed cups after 1h of rain (08:30-09:30). | Details in attached excel file. Air handler off during the rain.
2020-07-16 | 12h rain event (8:30-20:30), Multi 1, East hillslope. | Air handlers were turned off during rain. Mast lowered after the rain event.
| WEST |
2020-07-20 | Spanned ropes on West hillslope to mark cup locations for rainfall calibration. | Masts were raised in the morning. Kept raised until after the 12h rain event. Ropes spanned upslope-downslope with pre-labeled marks every 2m from 0-30m.
2020-07-21 | Placed cups on West hillslope and removed ropes. |
2020-07-22 | Rainfall calibration, Multi 1, West hillslope. Collected and weighed cups after 1h of rain (08:30-09:30). | Details in attached excel file. Air handler off during the rain. Gantry malfunction caused an interruption of several hours during the cup collection.
2020-07-23 | 12h rain event (8:30-20:30), Multi 1, West hillslope. | Air handlers were turned off during rain. Mast lowered after the rain event.

After the experiment, cups, labeled ropes and cardboard transport boxes used for the cup collection during the rainfall calibration were stored in upper habitat office 10.

0
Tags:
Created by Hannes Bauser on 2022/05/03 16:48

- Attachments (1)
- History

# Quick Links

Biosphere2 Wiki Home

Landscape Evolution Observatory
- Data
- Irrigation
- Instrumentation
- Data-logging & Control
- Protocols & Walkthroughs
- Science Meetings
- Isotope Lab
- Missing Data

Mini LEO

Tropical Rain Forest
- Data-logging

Outside Weather
- Data-Logging
- Weather Underground

Ocean

# Blog Categories

- https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/">All

- Data-logging and Controls (34)
- Experiments (10)
  - bigPERTH_Soil Coring_After First Rainfall Pulse (2)
- Facilities (4)
- Irrigation (16)
- LEO (78)
- Mini LEO (8)
- News (2)
- Ocean (0)
- Other (2)
- Personal (0)
- TRF (0)

# Blog Archive

- 2009 (1)
- 2012 (4)
- 2013 (3)
- 2015 (22)
- 2016 (15)
- 2017 (4)
- 2018 (8)
- 2019 (9)
- 2020 (11)
- 2021 (5)
- 2022 (5)
- 2023 (4)
- 2024 (5)
- 2025 (1)
- 2026 (1)
  - February (1)

# Recent Blog Posts

- Novalynx Tipping Bucket Issue

- LEO Irrigation issues

- RO Filter Information

- West bay DVI7911 replacement

- West bay SDI12 power supply replaced

- West bay CSAT3 reinstall

- LEO center 5TM MPS2 sensor array offline

- CSAT3 redeployment

- EX81 flow meters zero reset

- Biweekly rain modification due to power fluctuation

# Blog Categories

- https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/">All

- Data-logging and Controls (34)
- Experiments (10)
  - bigPERTH_Soil Coring_After First Rainfall Pulse (2)
- Facilities (4)
- Irrigation (16)
- LEO (78)
- Mini LEO (8)
- News (2)
- Ocean (0)
- Other (2)
- Personal (0)
- TRF (0)

# Blog Archive

- 2009 (1)
- 2012 (4)
- 2013 (3)
- 2015 (22)
- 2016 (15)
- 2017 (4)
- 2018 (8)
- 2019 (9)
- 2020 (11)
- 2021 (5)
- 2022 (5)
- 2023 (4)
- 2024 (5)
- 2025 (1)
- 2026 (1)
  - February (1)

# All Blogs

- Blog

This wiki is licensed under a Creative Commons 2.0 license
XWiki Enterprise 13.10.5 - Documentation