# Blog

Last modified by Administrator on 2022/05/11 13:16
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20steady%20state%20experiment%201">

## Feb 19 2013

Feb 19, 2013,

### https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20steady%20state%20experiment%201">LEO-E steady state experiment 1

At approximately 10:00 MST on February 18, 2013, irrigation circuit Multi2 was activated to initiate the steady state rain experiment.
At approximately 7:45 MST on February 19, 2013, irrigation was stopped.

https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20wetting%20on%202013-01-25">

## Jan 25 2013

Jan 25, 2013,

### https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20wetting%20on%202013-01-25">LEO-E wetting on 2013-01-25

Jan. 25, 2013 From 10:50 to 17:50 (MST) irrigation circuit Multi2 (E) was run.
Recorded flow rate was approximately 1.13 liters per second - 7100 liters total

https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20rain%20drop%20analysis">

## Jan 02 2013

Jan 2, 2013,

### https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20rain%20drop%20analysis">LEO-E rain drop analysis

On 1/2/13 between approx 10 am and 12:30 pm, rain drop diameter and velocity distributions were measured on LEO1 slope. Measurements were acquired at two locations (upper and lower slope along central axis) for each rain circuit and then for all circuits simultaneously for 5 minutes at each setting.
(Notes from Jon Pelletier)

https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20irrigation%20testing">

## Nov 19 2012

Nov 19, 2012,

### https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20irrigation%20testing">LEO-E irrigation testing

On December 19, 2012 starting at 8:30am a series of irrigation tests were preformed. This test was designed to characterize the irrigation pattern (distribution of water) over the surface of the hill slope.
Test#1 - Irrigation circuit A "MP2000" 30 minutes
-> Flow rate 0.282176 liters per second
Test#2 - Irrigation circuit B "Interm" 40 minutes
-> Flow rate = 0.228867 liters per second
Test#3 - Irrigation circuit C "MP3000" 30 minutes
-> Flow rate = 0.649184 liters per second
Test#4 - Irrigation circuit D "Multi1" 30 minutes
-> Flow rate = 1.48213 liters per second
Test#5 - Irrigation circuit E "Multi2" 30 minutes
-> Flow rate = 0.765027 liters per second

https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20wetting%20on%202012-11-14">

## Nov 14 2012

Nov 14, 2012,

### https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20wetting%20on%202012-11-14">LEO-E wetting on 2012-11-14

At approximately 10:30 on Dec. 14, 2012 a rain event was started using the MP2000 (A) and Interm (B) irrigation circuits on the west half of the east hill slope (negative cross slope area).
At approximately 14:35 on Dec. 14, 2012 the rain event was ended.
Inbound flow rate is unknown and was not logged.

https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20wetting%20on%202012-11-05">

## Nov 05 2012

Nov 5, 2012,

### https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/LEO-E%20wetting%20on%202012-11-05">LEO-E wetting on 2012-11-05

Monday, Nov. 5, 2012: Rain event started at 11:30 AM - ended at 4:50PM
Irrigation valves open: A,B,C,D (MP2000, Interm, MP3000, Multi1)
Reported flow rate: 1.87 liters / second

https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/11-02-2012%20East%20irrigation%20test">

## Nov 02 2012

Nov 2, 2012,

### https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/11-02-2012%20East%20irrigation%20test">East irrigation test on 2012-11-02

Friday, Nov 2, 2012 @ 12:15 irrigation started - 14:15 irrigation stopped. Rain for two hours: Int, Multi 2, MP2000 (ABE).
Recorded flow rate: 1.2 liters per second
approx 8640 liters were applied, load cells indicated 8500kg wight change, this indicates a total depth of 2.6 cm for two hours.

https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/BlogIntroduction">
Jun 1, 2009,

### https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/BlogIntroduction">First blog post

This is your wiki's blog first post. Its goal is to provide a short description of your blog's main features.

- You can create new blog posts through the input field located on your Blog's homepage. The status of a blog post may be any one of the following:
  - Unpublished: your post is still a draft. It can be seen by its creator and by administrators. Once you have clicked publish, you cannot unpublish a post. However, you can choose to hide it.
  - Published: your post can be read by every user that has access to your blog.
  - Published & hidden: your post is published but only its creator and admins can see it. This is useful if you need to make modifications on a post that has already been published by mistake.

- Every blog article can be tagged and/or categorized:
  - You will be able to browse posts by category using the panel located on the left of the page
  - You can create new categories and subcategories when creating a new post
  - The use of tags allows your article to be found by browsing your wiki's tags, along with any other wiki document

- Blog-specific panels are available on the left of your blog page:
  - The recent posts lists the most recent entries to any visitor of the blog
  - The unpublished panel lists the blog posts you created, but didn't yet publish
  - The categories panel lets you browse blog posts listed by category and subcategory
  - The archive panel lets you browse blog posts by publication date

Happy blogging!

Newer posts »
0
Tags:
Created by Michael Sibayan on 2022/05/03 16:48

- Attachments (0)
- History

# Quick Links

Biosphere2 Wiki Home

Landscape Evolution Observatory
- Data
- Irrigation
- Instrumentation
- Data-logging & Control
- Protocols & Walkthroughs
- Science Meetings
- Isotope Lab
- Missing Data

Mini LEO

Tropical Rain Forest
- Data-logging

Outside Weather
- Data-Logging
- Weather Underground

Ocean

# Blog Categories

- All

- Data-logging and Controls (34)
- Experiments (10)
  - bigPERTH_Soil Coring_After First Rainfall Pulse (2)
- Facilities (4)
- Irrigation (16)
- LEO (78)
- Mini LEO (8)
- News (2)
- Ocean (0)
- Other (2)
- Personal (0)
- TRF (0)

# Blog Archive

- 2009 (1)
- 2012 (4)
- 2013 (3)
- 2015 (22)
- 2016 (15)
- 2017 (4)
- 2018 (8)
- 2019 (9)
- 2020 (11)
- 2021 (5)
- 2022 (5)
- 2023 (4)
- 2024 (5)
- 2025 (1)
- 2026 (1)
  - February (1)

# Recent Blog Posts

- Novalynx Tipping Bucket Issue

- LEO Irrigation issues

- RO Filter Information

- West bay DVI7911 replacement

- West bay SDI12 power supply replaced

- West bay CSAT3 reinstall

- LEO center 5TM MPS2 sensor array offline

- CSAT3 redeployment

- EX81 flow meters zero reset

- Biweekly rain modification due to power fluctuation

# Blog Categories

- All

- Data-logging and Controls (34)
- Experiments (10)
  - bigPERTH_Soil Coring_After First Rainfall Pulse (2)
- Facilities (4)
- Irrigation (16)
- LEO (78)
- Mini LEO (8)
- News (2)
- Ocean (0)
- Other (2)
- Personal (0)
- TRF (0)

# Blog Archive

- 2009 (1)
- 2012 (4)
- 2013 (3)
- 2015 (22)
- 2016 (15)
- 2017 (4)
- 2018 (8)
- 2019 (9)
- 2020 (11)
- 2021 (5)
- 2022 (5)
- 2023 (4)
- 2024 (5)
- 2025 (1)
- 2026 (1)
  - February (1)

# All Blogs

- Blog

This wiki is licensed under a Creative Commons 2.0 license
XWiki Enterprise 13.10.5 - Documentation