# CameraTrack

Last modified by Aaron Bugaj on 2022/05/03 16:48
Export
Office Formats
Export as PDF
Other Formats
Export as HTML

Between Spring 2015 and 2016, three camera track systems were installed in the LEO Hill-slope bays. Each track is mounted into the space frame above the Hill-slope via all-thread and unistrut supports. Additionally, guide wires branch out from the track system and connect to the frame to limit swaying.

Macron Track Systems Assembly Instructions for West and Center Hillslopes:

ASSEMBLY INSTRUCTIONS.pdf

0
Tags:
Created by Aaron Bugaj on 2022/05/03 16:48

- Attachments (1)
- History

# Quick Links

Biosphere2 Wiki Home

Landscape Evolution Observatory
- Data
- Irrigation
- Instrumentation
- Data-logging & Control
- Protocols & Walkthroughs
- Science Meetings
- Isotope Lab
- Missing Data

Mini LEO

Tropical Rain Forest
- Data-logging

Outside Weather
- Data-Logging
- Weather Underground

Ocean

# Blog Categories

- https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/">All

- Data-logging and Controls (33)
- Experiments (10)
  - bigPERTH_Soil Coring_After First Rainfall Pulse (2)
- Facilities (4)
- Irrigation (16)
- LEO (77)
- Mini LEO (8)
- News (2)
- Ocean (0)
- Other (2)
- Personal (0)
- TRF (0)

# Blog Archive

- 2009 (1)
- 2012 (4)
- 2013 (3)
- 2015 (22)
- 2016 (15)
- 2017 (4)
- 2018 (8)
- 2019 (9)
- 2020 (11)
- 2021 (5)
- 2022 (3)
- 2023 (1)
- 2024 (1)

# Recent Blog Posts

- LEO Irrigation issues

- RO Filter Information

- West bay DVI7911 replacement

- West bay SDI12 power supply replaced

- West bay CSAT3 reinstall

- LEO center 5TM MPS2 sensor array offline

- CSAT3 redeployment

- EX81 flow meters zero reset

- Biweekly rain modification due to power fluctuation

- Rain schedule post CRQ experiment

# Recently Modified

- LEO Irrigation issues
- RO Filter Information
- Profile of Rhiannon Nabours
- Rain schedule post CRQ experiment
- West bay DVI7911 replacement

This wiki is licensed under a Creative Commons 2.0 license
XWiki Enterprise 13.10.5 - Documentation