# Irrigation System

Last modified by Aaron Bugaj on 2022/05/03 16:48
Export
Office Formats
Export as PDF
Other Formats
Export as HTML

Table of contents

- Irrigation circuits
- Irrigation Scenarios
- Irrigation Control
- Water storage

Each hill slope was designed with five (5) irrigation circuits. Each hill slope is fed via a supply line which can be charged using any of the pumps (valving restrictions apply)

# Irrigation circuits

Circuit A (MP2000)
- This circuit utilizes six (8) Hunter MP2000 heads providing approximately 0.32 cm/hr of rain

Circuit B (Intermediate)
- This circuit utilizes eight (6) Hunter MP2000 heads providing approximately 0.31 cm/hr of rain

Circuit C (MP3000)
- This circuit utilizes eight (8) Hunter MP3000 heads providing approximately 0.74 cm/hr of rain

Circuit D (Multi1)
- This circuit utilizes fourteen (14) Hunter MP2000 heads and fourteen (8) Hunter MP3000 heads providing approximately 1.37 cm/hr of rain

Circuit E (Multi2)
- This circuit utilizes fourteen (14) Hunter MP2000 heads and fourteen (8) Hunter MP3000 heads providing approximately 1.37 cm/hr of rain

*** Please note ***
Circuit D and E are designed to be identical and each is equivalent to the combination of A + B + C.

# Irrigation Scenarios

A (MP2000) | B (Interm) | C (MP3000) | D (Multi1) | E (Multi2) | Rain Rate (cm/hr) | scenario #
|  |  |  |  | 0.00 | 0
X |  |  |  |  | 0.31 | 1
| X |  |  |  | 0.32 | 2
X | X |  |  |  | 0.63 | 3
|  | X |  |  | 0.74 | 4
X |  | X |  |  | 1.05 | 5
| X | X |  |  | 1.06 | 6
|  |  | X |  | 1.37 | 7
X |  |  | X |  | 1.68 | 8
| X |  | X |  | 1.69 | 9
X | X |  | X |  | 2.00 | 10
|  | X | X |  | 2.11 | 11
X |  | X | X |  | 2.42 | 12
| X | X | X |  | 2.43 | 13
|  |  | X | X | 2.74 | 14
X |  |  | X | X | 3.05 | 15
| X |  | X | X | 3.06 | 16
X | X |  | X | X | 3.37 | 17
|  | X | X | X | 3.48 | 18
X |  | X | X | X | 3.79 | 19
| X | X | X | X | 3.80 | 20
X | X | X | X | X | 4.11 | 21

# Irrigation Control

Each of the five irrigation circuits is operated by a VALWORX electric ball valve. These valves can be opened and closed manually or by computer control. The device cRIO-LEO-Irrigation (located in the irrigation electrical control panel) is configured as a task scheduler which provides the ability to precisely automate complex valve action scenarios. More information regarding this topic can be found in the page IRRIGATION CONTROL

# Water storage

There are 7 tank in the east bay - each tank can hold approximately 8,037 Liters.
There are 4 tank in the west bay - each tank can hold approximately 9,690 liters.
The RO can produce approximately 75 liters per minute.

East bay storage tanks, pipes & valving shown in the image below:

0
Tags:
Created by Michael Sibayan on 2022/05/03 16:48

- Attachments (3)
- History

# Quick Links

Biosphere2 Wiki Home

Landscape Evolution Observatory
- Data
- Irrigation
- Instrumentation
- Data-logging & Control
- Protocols & Walkthroughs
- Science Meetings
- Isotope Lab
- Missing Data

Mini LEO

Tropical Rain Forest
- Data-logging

Outside Weather
- Data-Logging
- Weather Underground

Ocean

# Blog Categories

- https://wiki.b2.arizona.edu/xwiki/bin/view/Blog/">All

- Data-logging and Controls (33)
- Experiments (10)
  - bigPERTH_Soil Coring_After First Rainfall Pulse (2)
- Facilities (4)
- Irrigation (16)
- LEO (77)
- Mini LEO (8)
- News (2)
- Ocean (0)
- Other (2)
- Personal (0)
- TRF (0)

# Blog Archive

- 2009 (1)
- 2012 (4)
- 2013 (3)
- 2015 (22)
- 2016 (15)
- 2017 (4)
- 2018 (8)
- 2019 (9)
- 2020 (11)
- 2021 (5)
- 2022 (3)
- 2023 (1)
- 2024 (1)

# Recently Visited

- Mini LEO PE102 and Tipping bucket calculation change
- Irrigation System

# Recent Blog Posts

- LEO Irrigation issues

- RO Filter Information

- West bay DVI7911 replacement

- West bay SDI12 power supply replaced

- West bay CSAT3 reinstall

- LEO center 5TM MPS2 sensor array offline

- CSAT3 redeployment

- EX81 flow meters zero reset

- Biweekly rain modification due to power fluctuation

- Rain schedule post CRQ experiment

# Recently Modified

- LEO Irrigation issues
- RO Filter Information
- Profile of Rhiannon Nabours
- Rain schedule post CRQ experiment
- West bay DVI7911 replacement

This wiki is licensed under a Creative Commons 2.0 license
XWiki Enterprise 13.10.5 - Documentation